How to set Anti-Passback:

Make sure all your controllers connect to 1 switch board to make sure signal stable.

1, add the controller



2, Click “anti-passback”

Press: ctrl+shift+Q

You will see: Active Anti-Passback Siganl sahre ( All Controllers in the same subnet)

Click this.

Then click the 10 pcs controller and click NO1 / NO2 each other.



3, After you set all these 10 controller, then select these 10 controller’s door, then “upload”

